# DSP.C5x[x].Libs[y]

Specifies the DSP library file name.

#### Syntax

DSP.C5x[x].Lib[y] = filename

x = 0-(n-1) (A range of DSP cores where n equals the total number of DSP cores available.)

y = 0..15 (index of a DSP library)

#### Access

Read/Write

#### Type

File name

#### Default

cg6kliba

#### Allowed values

A valid DSP library file name.

#### Example

DSP.C5x[0..19].Lib[0] = cg6kliba.r54

#### Details

There are two DSP operating system service libraries: cg6klibu.r54 and cg6kliba.r54.

Library | Function
--- | ---
cg6kliba | A-law conversion
cg6klibu | mu-law conversion

Note: All DSPs must be set to either A-law
or mu-law
.

#### See also

DSP.C5x[x].OS, DSP.C5x[x].NumRxTimeSlots, DSP.C5x[x].NumTxTimeSlots, DSP.C5x[x].XLaw