# AutoStartEnabled

If set to Yes, the Supervisor attempts to start all boards whenever it starts up or when a board is Hot Swap-inserted.

#### Syntax

AutoStartEnabled = flag

#### Access

Read/Write

#### Type

String

#### Default

No

#### Allowed values

Yes | No

#### Example

AutoStartEnabled = No

#### Details

The Supervisor starts a board automatically only if the AutoStart keyword in the board's managed object is set to Yes.

For more information about starting boards automatically, refer to the NMS OAM System User's Manual.

#### See also

AutoStopEnabled