# AutoStopEnabled

If set to Yes, the Supervisor attempts to stop all boards whenever it shuts down.

#### Syntax

AutoStopEnabled = flag

#### Access

Read/Write

#### Type

String

#### Default

No

#### Allowed values

Yes | No

#### Example

AutoStopEnabled = No

#### Details

The Supervisor stops a board automatically only if the AutoStop keyword in the board's managed object is set to Yes.

For more information about stopping boards automatically, refer to the NMS OAM System User's Manual.

#### See also

AutoStartEnabled